****

**INVITATION TO BID**

**FOR THE CONSTRUCTION OF FCMD FIELD OFFICE INTO ONE STOP SHOP PORT OPERATION BUILDING, PORT OF DAPITAN, DAPITAN CITY, ZAMBOANGA DEL NORTE**

The Philippine Ports Authority, PMO- Zamboanga del Norte, through its bids and Awards Committee for Infrastructure Projects intends to apply the sum of **12,021,827.41** being the Approved Budget for the Contract (ABC) to payment under the contract for the CONSTRUCTION OF FCMD FIELD OFFICE INTO ONE STOP SHOP PORT OPERATION BUILDING, PORT OF DAPITAN, DAPITAN CITY, ZAMBOANGA DEL NORTE. Bids received in excess of the ABC shall be automatically rejected at Bid Opening.

The PPA, PMO-Zamboanga del Norte, through its Bids and Awards Committee for Infrastructure Projects now invites bids for the project with the following scope of work:

1. **Scope of Work:**

|  |  |  |  |
| --- | --- | --- | --- |
| **NO.** | **DESCRIPTION OF WORK** | **QTY.** | **UNIT** |
|   |   |   |   |
| (1) | (2) | (3) | (4) |
| **1.0** | **General Expenses** |  |  |
| 1.1 | Mobilization/Demobilization | 1 | lot |
| 2.1 | Construction safety & health program | 1 | lot |
| **2.0** | **Demolition/Excavation Works** |  |  |
| 2.1 | Demolish, remove & dispose existing pav't. for | 228 | sq.m. |
|  | ftgs., tie beams, septic tank, drainage system |  |  |
|  | catch basin. |  |  |
| 2.2 | Demolish, Remove & Dispose Existing FCMD Building | 60 | sq.m. |
| 2.3 | Excavate and dispose excess materials for ftgs | 140 | cu.m. |
|  | tie beams, septic tank, catch basis & drainage System |  |  |
| **3.0** | **Filling Materials** |  |  |
| 3.1 | Spread and Compact Filling Materials | 386 | cu.m. |
| **4.0** | **Concreting Works** |  |  |
| 4.1 | Supply, Fab. & Install Steel Reinforcement | 27,113 | kgs. |
| 4.2 | Concreting of Structural Members & Slabs | 175 | cu.m. |
| 4.3 | Construction of Septic Tank | 1 | lot |
| **5.0** | **Masonry Works** |  |  |
| 5.1 | Supply & Install/Laying of 100mm thk. CHB | 392 | sq.m. |
| 5.2 | Plastering and Finishing of Concrete Walls | 272 | sq.m. |
| 5.3 | Plastering and Finishing of Concrete Walls | 1,328 | sq.m. |
| **6.0** | **Roofing Works** |  |  |
| 6.1 | Supply, Fab. & Install Pre-Painted Twin-Rib | 323.00 | sq.m. |
|  | G.I. Roofing Sheets and Accessories |  |  |
| 6.2 | Supply, Fab. & Install Angular Steel Bar | 21 | Sets |
| 6.3 | Supply, Fab. & Install Steel C-Purlins | 528 | l.m. |
| 6.4 | Supply & Install PVC Downspout | 58 | l.m. |
| **7.0** | **Finishes and Fixtures** |  |  |
| 7.1 | Supply & Install 200mm x 200mm Unglazed | 33 | sq.m. |
|  | Ceramic Tiles for Comfort Rooms |  |  |
| 7.2 | Supply & Install 200mm x 300mm Glazed | 121 | sq.m. |
|  | Ceramic Wall Tiles for Comfort Rooms |  |  |
| 7.3 | Supply & Install 600mm x 600mm Glazed | 362 | sq.m. |
|  | Semi-Granite Floor Tiles |  |  |
| 7.4 | Supply & Install Water Closets complete w/ | 6 | sets |
|  | Fittings and Accessories |  |  |
| 7.5 | Supply & Install Wall-Hung Lavatory complete | 10 | sets |
|  | w/ Fittings and Accessories |  |  |
| 7.6 | Supply & Install Wall-Hung Urinals complete | 5 | sets |
|  | w/ Fittings and Accessories |  |  |
| **8.0** | **Installation of Doors and Windows** |  |  |
| 8.1 | Supply & Install Double Swing Tempered | 2 | sets |
|  | Glass Door on Powder Coated Alum. Frame |  |  |
| 8.2 | Supply & Install Panel Type Tempered Frame- | 13 | sets |
|  | less Glass Door |  |  |
| 8.3 | Supply & Install Sliding Tempered Glass Window | 10 | sets |
|  | on Powder Coated Alum. Frame |  |  |
| 8.4 | Supply & Install Fixed Tempered Glass Window | 33 | sets |
|  | on Powder Coated Alum. Frame |  |  |
| 8.5 | Supply & Install Awning Type Tempered Glass | 13 | sets |
|  | Window on Powder Coated Alum. Frame |  |  |
| 8.6 | Supply & Install Pre-Fabricated Laminated | 6 | sets |
|  | Door w/ Wooden Door Frame |  |  |
| 8.7 | Supply & Install Heavy Duty Louver Type PVC | 7 | sets |
|  | Door w/ PVC Door Frame |  |  |
| **9.0** | **Plumbing Works** |  |  |
| 9.1 | Supply & Install 100mm dia. PVC Pipe | 39.00 | l.m. |
| 9.2 | Supply & Install 75mm dia. Secondary PVC Pipe | 34.00 | l.m. |
| 9.3 | Supply & Install 50mm dia. PVC Pipe | 58.00 | l.m. |
| 9.4 | Supply & Install 50mm dia. uPVC Pipe Moldex | 96 | l.m. |
|  | Blue Pipe for Water Supply Line |  |  |
| **10.0** | **Electrical Works** |  |  |
| 10.1 | Supply & Install THW Stranded Wire | 2,510 | l.m. |
| 10.2 | Supply & Install Ceiling Mounted Pinlight & | 74 | sets |
|  | Louver Type Flourescent Lamp |  |  |
| 10.3 | Supply & Install Flush Type Convenience & | 44 | sets |
|  | Aircon Outlets |  |  |
| 10.4 | Supply & Install Ceiling and Wall Mounted Exhaust Fan | 11 | units |
| 10.5 | Supply & Install Flush Type Switch | 33 | sets |
| 10.6 | Supply & Install Circuit Breakers and Panel Board | 19 | sets |
| **11.0** | **Ceiling Works** |  |  |
| 11.1 | Supply & Install 9.50mm thk. x 600 x 600mm | 164.00 | sq.m. |
|  | Laminated Gypsum Elefoil Ceiling Board |  |  |
| 11.2 | Supply & Install 9.50mm thk. x 600 x 600mm | 237.00 | sq.m. |
|  | Acoustic Ceiling Board |  |  |
| 11.3 | Supply & Install Rib-3 Spanflex Steel for Eaves | 131.00 | sq.m. |
| **12.0** | **Painting Works** |  |  |
| 12.1 | Painting of Steel Surfaces | 288.00 | sq.m. |
| 12.2 | Painting of Concrete/Masonry Surfaces | 1,328.00 | sq.m. |
| 12.3 | Painting of Wooden Surfaces | 35.00 | sq.m. |
| **13.0** | **Drainage System** |  |  |
| 13.1 | Construction of Catch Basin | 8 | units |
| 13.2 | Construction of Reinforced Concrete Canal | 15 | l.m. |
| 13.3 | Supply, Fabricate & Install Steel Grating Cover | 15 | l.m. |
| 13.4 | Supply & Install PVC Pipe | 32 | l.m. |
| **14.0** | **Fire Protection System** |  |  |
| 14.1 | Supply & Install G.I. Pipe Lines & Sprinklers | 150 | l.m. |

**B. List of Equipments**

|  |  |  |  |
| --- | --- | --- | --- |
| 1.0. | Concrete Saw/Cutter (Gasoline) w/ 12" Blade | 1 | Unit |
| 2.0. | Backhoe (.50 cu.m. Cap.) 110HP | 1 | Unit |
| 3.0. | Dump Truck (6-8.99 cu.m. Cap.) 220HP | 1 | Unit |
| 4.0. | Vibratory Plate Compactor (Gasoline Engine) 6-8HP  | 1 | Unit |
| 5.0. | Welding Machine w/ Complete Acc. (ED-300A) | 1 | Unit |
| 6.0. | Rebar Bender (16mm)  |   | 1 | Unit |
| 7.0. | Rebar Cutter (16mm) |   | 1 | Unit |
| 8.0. | One Bagger Concrete Mixer |   | 1 | Unit |
| 9.0. | Concrete Vibrator 2" Flexible Shaft | 1 | Unit |
| 10.0. | Water Truck (500-1,000 Gals. Capacity) | 1 | Unit |
| 11.0 | Electric Grinder | 1 | Unit |
| 12.0 | Electric Hand Drill | 1 | Unit |
| 13.0 | Tile Cutter | 1 | Unit |
| 14.0 | Oxy-Accetylene Cutter w/ complete Accessories | 1 | Unit |

Completion of the works is required **240 Calendar Days**. Bidders must have an experience of having completed at least one (1) contract that is similar to the contract to be bid, and whose value, adjusted to the current prices, must be at least 50% of the approved budget for the contract to be bid.

Bidding will be conducted through open competitive bidding procedures using non-discretionary pass/fail criterion as specified in the Implementing Rules and Regulations of Republic Act 9184 (RA 9184), otherwise known as the “Government Procurement Reform Act”.

Bidding is restricted to Filipino citizens/Sole proprietorships, partnerships, or organizations with at least seventy five percent (75%) interest or outstanding capital stock belonging to citizens of the Philippines and with Minimum PCAB License Registration-Small B - Building & Industrial Plant.

Interested bidders may obtain further information from PPA, PMO-Zamboanga del Norte and inspect the Bidding Documents at the address given below from 8:00AM to 5:00PM, Monday to Friday.

Letter of Intent will be received from April 18-25, 2016. Only Letter of Intent (LOI) with attached 1- xerox copy of PCAB License will be accepted. Please present Original Copy of PCAB License at the time of submission of LOI for verification purposes. Bidders without similar experience to the contract to be bid need not apply.

A complete set of Bidding Documents may be purchased by interested bidders from the address below and upon payment of a non-refundable fee for the Bidding Documents in the amount of Twenty Five Thousand Pesos (Php 25,000.00), exclusive of VAT.

The PPA, PMO-Zamboanga del Norte will hold a Pre-Bid conference on April 26, 2016, 2:00PM at PPA Conference Room, Admin. Bldg.,Port of Dapitan, which shall be open only to all interested parties who have purchased the Bidding Documents.

Bids must be delivered to the address below on or before May 11, 2016, 10:00 AM at PPA Conference Room, PMO-Zamboanga del Norte, Port area, Dapitan city address to the BAC Chairman for Infrastructure Projects. All bids must be accompanied by a bid security in any of the acceptable forms and in the amount stated in the Instruction to Bidders. Bids will be opened in the presence of the bidder’s representatives who choose to attend at the address below. Late bids shall not be accepted.

The PPA, PMO-Zamboanga del Norte reserves the right to accept or reject any bid, to annul the bidding process, and to reject all bids at any time prior to contract award, without thereby incurring any liability to the affected bidder or bidders.

**ENGR. ABDURASAD S. HASAN**

BAC Chairperson for Infrastructure Projects

PPA, PMO-Zamboanga del Norte, Port Area, Dapitan City 7101

For further information, please refer to:

The BAC Secretariat for Infrastructure Projects or The ESD Office

PPA, PMO-Zamboanga del Norte, Port Area, Dapitan City 7101

Tel No. (065) 213-6595, (065) 213-6946

Email Address:ppa.pmo.dapitan@gmail.com

Date of Publication: April 18-25, 2016

PPA Website: www.ppa.com.ph

PhilGeps Website: www.philgeps.net

Philippine Star (Newspaper) April 18, 2016